 - ______________________________ 
 - Cockpit Inspection  - 
 
[ ] - Wheel Brake  - ON  (Throttle panel)
[ ] - Master Battery - ON  (Overhead panel)
[ ] - Panel lights - AS REQUIRED  (Overhead panel)
[ ] - Nav. Lights - ON  (Overhead panel)
[ ] - Left and right condition levers - FUEL SHUTOFF  (Throttle panel)
 - ______________________________ 
 - Start in hotel mode-(cold start)  - 
 
[ ] - Propeller brake switch - ON  (Overhead panel)
[ ] - Propeller brake indicator  - INDICATES READY  (Overhead panel)
[ ] - Beacon light - ON  (Overhead panel)
[ ] - Starter selector - CRANK  (Overhead panel)
[ ] - Engine #2 starter - ACTIVATE   (Overhead panel)
[ ] - Starter selector - START A + B  (Overhead panel)
[ ] - Engine #2 starter - ACTIVATE   (Overhead panel)
[ ] - Engine #2 N1  - 10% OR MORE  (Main panel)
[ ] - Engine #2 condition lever - FEATHER  (Trhottle panel)
[ ] - Engine #2 EGT - GREEN ARC  (Main panel)
[ ] - Sarter selector - OFF  (Overhead panel)
[ ] - Generator #2 fail indicator - EXTINGUISHED  (Overhead panel)
[ ] - Generator #2 breaker - ON  (Overhead panel)
[ ] - Generator #2 annunciator (CCAS) - EXTINGUISHED  (Main panel)
 - ______________________________ 
 - Start in hotel mode (hot start)  - 
 
[ ] - Propeller brake switch - ON  (Overhead panel)
[ ] - Propeller brake indicator  - INDICATES READY  (Overhead panel)
[ ] - Beacon light - ON  (Overhead panel)
[ ] - Starter selector - START A  OR START B  (Overhead panel)
[ ] - Engine #2 starter - ACTIVATE   (Overhead panel)
[ ] - Engine #2 N1  - 10% OR MORE  (Main panel)
[ ] - Engine #2 condition lever - FEATHER  (Trhottle panel)
[ ] - Engine #2 EGT - GREEN ARC  (Main panel)
[ ] - Sarter selector - OFF  (Overhead panel)
[ ] - Generator #2 fail indicator - EXTINGUISHED  (Overhead panel)
[ ] - Generator #2 breaker - ON  (Overhead panel)
[ ] - Generator #2 annunciator (CCAS) - EXTINGUISHED  (Main panel)
 - ______________________________ 
 - Instrumentation & Configuration  - 
 
[ ] - Avionics switch - ON  (Overhead panel)
[ ] - H S I - CONFIGURE  (Main Panel)
[ ] - Autopilot - SET UP FOR FLIGHT  (Main Panel)
[ ] - IAS hold speed (Airspeed indicator) - SET UP FOR CLIMB (160KIAS)  (Main Panel)
 - ______________________________ 
 - Engine#2 propeller start  - 
 
[ ] - Engine #2 Power lever - IDLE  (Throttle panel)
[ ] - Engine#2 condition lever - FEATHER  (Throttle panel)
[ ] - Propeller brake indicator - REEADY  (Overhead panel)
[ ] - Propeller area - CLEAR  ()
[ ] - Propeller brake switch - OFF  (Overhead panel)
[ ] - Engine#2 rpm - SHOWS POSITIVE READING  (Main panel)
[ ] - Engine #2 condition lever - FULL RPM AFTER 10 SECONDS  (Throttle panel)
[ ] - Propeller brake indicator - EXTINGUISHED  (Overhead panel)
 - ______________________________ 
 - Engine #1 start (cold start)  - 
 
[ ] - Starter selector - CRANK  (Overhead panel)
[ ] - Propeller area - CLEAR  ()
[ ] - Engine #1 starter - ACTIVATE   (Overhead panel)
[ ] - Starter selector - START A + B  (Overhead panel)
[ ] - Engine #1 starter - ACTIVATE   (Overhead panel)
[ ] - Engine #1 N1  - 10% OR MORE  (Main panel)
[ ] - Engine #1 condition lover - FEATHER  (Trhottle panel)
[ ] - Engine #1 EGT - GREEN ARC  (Main panel)
[ ] - Sarter selector - OFF  (Overhead panel)
[ ] - Engine #1 condition lover - FULL RPM AFTER 10 SECONDS  (Trhottle panel)
[ ] - Generator #1 fail indicator - EXTINGUISHED  (Overhead panel)
[ ] - Generator #1 breaker - ON  (Overhead panel)
[ ] - Generator #1 annunciator (CCAS) - EXTINGUISHED  (Main panel)
 - ______________________________ 
 - Engine #1 start (hot start)  - 
 
[ ] - Propeller area - CLEAR  ()
[ ] - Starter selector - START A  OR START B  (Overhead panel)
[ ] - Engine #1 starter - ACTIVATE   (Overhead panel)
[ ] - Engine #1 N1  - 10% OR MORE  (Main panel)
[ ] - Engine #1 condition lover - FEATHER  (Trhottle panel)
[ ] - Engine #1 EGT - GREEN ARC  (Main panel)
[ ] - Sarter selector - OFF  (Overhead panel)
[ ] - Engine #1 condition lever - FULL RPM AFTER 10 SECONDS  (Trhottle panel)
[ ] - Generator #1 fail indicator - EXTINGUISHED  (Overhead panel)
[ ] - Generator #1 breaker - ON  (Overhead panel)
[ ] - Generator #1 annunciator (CCAS) - EXTINGUISHED  (Main panel)
 - ______________________________ 
 - Pre-taxi  - 
 
[ ] - Flaps - SET 10º  (Throttle panel)
[ ] - Trim - TAKEOFF CONFIG  (Throttle panel)
[ ] - Taxi light - ON  (Overhead panel)
[ ] - Idle gate - GROUND IDLE  (Throttle panel)
[ ] - Parking brake  - RELEASE  (Throttle panel)
[ ] - Torque white bugs - ADJUST TO TAKEOFF TORQUE  (Main panel)
 - ______________________________ 
 - Before Takeoff  - 
 
[ ] - Flaps - CHECK 10º  (Main panel)
[ ] - Trim - CHECK TO CONFIG  (Main panel)
[ ] - Propeller brake - CHECK OFF  (Overhead panel)
[ ] - Taxi Lights - ON UPON CLEARANCE FOR TAKING RUNWAY  (Overhead panel)
[ ] - PMS selector - TO  (Main panel)
 - ______________________________ 
 - Takeoff  - 
 
[ ] -  Strobe Lights - ON  (Overhead panel)
[ ] - Pitot heat - ON  (Overhead panel)
[ ] - Landing lights - ON  (Overhead panel)
[ ] - Starter selector - CONTINOUS RELIGHT  (Overhead panel)
[ ] - Idle gate - FLIGHT IDLE  (Throttle panel)
[ ] - Condition levers - AUTO  (Throttle panel)
[ ] - Power levers - ADJUST TO TO TORQUE  (Throttle panel)
[ ] - Power management - BOTH ENGINES ON (Main Panel)
[ ] - Call airspeeds - 80 KIAS - AIRSPEED ACTIVE  (Main panel)
 -  - V1  (Main panel)
 -  - VR  (Main panel)
 -  - V2  (Main panel)
 - ______________________________ 
 - Climb Out  - 
 
[ ] - Positive Climb Rate -  - GEAR UP  (Main panel)
[ ] - Yaw damper - ENGAGE  (Main panel)
[ ] - Auto Pilot - ENGAGE  (Main panel)
[ ] - De-icing equipment - AS REQUIRED  (Overhead panel)
[ ] - PMS - SELECT CLB  (Main panel)
[ ] - Above VmLB 0 - SET FLAPS 0  (Throttle panel)
[ ] - Landing lights - OFF ABOVE 10000 FT  (Overhead panel)
[ ] - Above FL180 Altimeter - SET 29.92/1013.25   (Main panel)
 - ______________________________ 
 - Cruise  - 
 
[ ] - PWR MGT - SELECT CRZ AFTER REACHING CRUISE SPEED  (Main panel)
[ ] - Engine instrumentation - MONITOR  (Main panel)
[ ] - CCAS - MONITOR  (Main panel)
[ ] - De-icing equipment - AS REQUIRED  (Overhead panel)
 - ______________________________ 
 - Descent  - 

[ ] - Power management - BOTH ENGINES OFF  (Throttle panel) 
[ ] - Power levers - ADJUST TO NOT EXCEED 240 KIAS  (Throttle panel)
[ ] - Below FL180 Altimeter - SET 29.92/1013.25   (Main panel)
[ ] - Troque bugs - SET TO/GA TORQUE  (Main panel)
[ ] - Landing lights - ON BELOW 10000FT  (Overhead panel)
 - ______________________________ 
 - Final Descent  - 
 
[ ] - Power levers - FLIGHT IDLE  (Throttle panel)
[ ] - At 160 KIAS - SET FLAPS 15º  (Throttle panel)
[ ] - PWR MGT - SELECT TO  (Main panel)
[ ] - At 145 KIAS - SET FLAPS 30º  (Throttle panel)
[ ] - Condition levers - SET MAX RPM AT APPROACH SPEED  (Throttle panel)
[ ] - Power levers - ADJUST TO MAINTAIN APPROACH SPEED  (Throttle panel)
 - ______________________________ 
 - Pre-Landing  - 
 
[ ] - Autopilot - DISENGAGE  (Main panel)
[ ] - Yaw damper - DISENGAGE  (Main panel)
[ ] - Gear - CHECK DOWN AND LOCKED  (Main panel)
[ ] - Idle gate - GROUND IDLE  (Throttle panel)
 - ______________________________ 
 - Landing  - 
 
[ ] - Power levers - FLIGHT IDLE AT 20' AGL  (Throttle panel)
[ ] - Main gear touchdown - NOSE DOWN 
 - ______________________________ 
 - After Landing  - 
 
[ ] - Pitot heat - OFF  (Overhead panel)
[ ] - Landing lights - OFF  (Overhead panel)
[ ] - Taxi lights - AS REQUIRED  (Overhead panel)
[ ] - Strobe lights - OFF  (Overhead panel)
[ ] - Flaps - RETRACT 
 - ______________________________ 
 - Aircraft parking - Hotel mode  - 
 
[ ] - Power levers - GROUND IDLE  (Throttle panel)
[ ] - Wheel Brake  - ON  (Throttle panel)
[ ] - Taxi lights - OFF  (Overhead panel)
[ ] - Engine #1 condition lever - FUEL SHUTOFF  (Throttle panel)
[ ] - Generator #1 breaker - OFF  (Overhead panel)
[ ] - Engine #2 condition lever - FEATHER  (Throttle panel)
[ ] - Propeller brake UNLOCK indication - EXTINGUISHED  (Overhead panel)
[ ] - Propeller brake READY indication - ILLUMINATED  (Overhead panel)
[ ] - Propeller brake switch - ON  (Overhead panel)
[ ] - Propeller brake indicator - ON  (Overhead panel)
[ ] - Propeller 2 rpm - CONFIRM ZERO READING  (Main panel)
 - ______________________________ 
 - Aircraft shutdown  - 
 
[ ] - Avionics switch - OFF  (Overhead panel)
[ ] - Generator #2 breaker - OFF  (Overhead panel)
[ ] - Engine #2 condition lever - FUEL SHUTOFF  (Throttle panel)
[ ] - Propeller brake switch - OFF AFTER ENGINE SHUTDOWN  (Overhead panel)
[ ] - Nav. Lights - OFF  (Overhead panel)
[ ] - Wing Lights - OFF  (Overhead panel)
[ ] - Beacon light - OFF  (Overhead panel)
[ ] - Panel lights - OFF  (Overhead panel)
[ ] - Master Battery - OFF  (Overhead panel)

