INSTALLATION: HJG DC-8-62 & -63 SERIES PANEL (WITH INS)

PLEASE NOTE: This particular panel is intended to be used with "HJG DC-8-62 & -63" aircraft models.

This panel is configured with gauges specially calibrated for P&W JT3D-3B and P&W JT3D-7 series fanjet performance in conjunction with revised DC-8-62 & -63 FDE data.

This panel is for FS2004 and FSX.  It is not compatible with FS2002. 

Panel installation is very easy but please read the following instructions carefully. This is our recommended installation procedure :-

1. This folder contains a sub folder named "panel.DC8-62_63_INS". 

2. Simply install this entire folder "intact" inside your "FSFSCONV" folder .... you should find this folder located inside your FS2004 "AIRCRAFT" folder or FSX "SIMOBJECTS\AIRPLANES" folder.  If the folder does not exist you should create it.

3. To make this panel display with your aircraft model you must open the "PANEL" folder inside your HJG DC-8-62 & -63 aircraft. It will contain a notepad named "PANEL". Open this notepad and by default it should read as follows :-

[fltsim]
alias=B737_400\panel

4. Pay attention to the line "ALIAS=B737_400\PANEL". Change this line to read exactly as follows :-

alias=fsfsconv\panel.DC8-62_63_INS

The completed notepad entry will then look like this :-

[fltsim]
alias=fsfsconv\panel.DC8-62_63_INS

And that's it !

Enjoy flying the HJG DC-8 panel series. 

Mark CRANSTON

June 2010